Table S1: Level 1 classification results for the different datasets at each of the three study sites. BR – Mount Brandon, GT – Galtee Mountains, and CM – Comeragh Mountains.
	
	(i) Optical & texture
	(ii) Radar & texture
	(iii) Optical & texture & VIs
	(iv) Optical & ancillary data
	(v) Radar & ancillary data
	(vi) Optical & Radar
	(vii) Optical & Radar      (inc texture & VIs)
	(viii) Optical & Radar & ancillary data

	
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM

	Overall Accuracy (%)
	88.9
	89.8
	88.8
	66.7
	66.3
	70.9
	88.2
	89.9
	87.9
	94.5
	94.7
	94.7
	88.8
	86.1
	89.7
	89.8
	89.4
	89.3
	90.8
	90.8
	90.9
	95.0
	94.9
	95.2

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Improved Grassland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(GA)                               PA
	0.98
	0.98
	0.97
	0.69
	0.72
	0.74
	0.97
	0.97
	0.96
	0.98
	0.99
	0.99
	0.96
	0.94
	0.97
	0.98
	0.97
	0.96
	0.99
	0.98
	0.98
	0.99
	0.99
	0.98

	  UA
	0.97
	0.95
	0.97
	0.79
	0.79
	0.84
	0.96
	0.95
	0.97
	0.98
	1.00
	1.00
	0.94
	0.98
	0.99
	0.99
	0.96
	0.98
	0.98
	0.96
	0.98
	0.99
	1.00
	1.00

	Semi-improved grassland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(GS)                               PA
	0.94
	0.86
	0.84
	0.47
	0.48
	0.50
	0.93
	0.86
	0.82
	0.96
	0.95
	0.91
	0.86
	0.86
	0.86
	0.95
	0.87
	0.84
	0.95
	0.86
	0.85
	0.97
	0.94
	0.92

	UA
	0.96
	0.88
	0.83
	0.37
	0.20
	0.30
	0.95
	0.87
	0.82
	0.97
	0.90
	0.90
	0.75
	0.63
	0.78
	0.97
	0.86
	0.81
	0.96
	0.88
	0.83
	0.98
	0.90
	0.89

	Heath
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(HH)                               PA
	0.78
	0.84
	0.80
	0.54
	0.56
	0.50
	0.77
	0.84
	0.78
	0.90
	0.90
	0.88
	0.79
	0.79
	0.73
	0.80
	0.83
	0.77
	0.80
	0.85
	0.79
	0.90
	0.91
	0.89

	UA
	0.84
	0.88
	0.72
	0.70
	0.75
	0.55
	0.83
	0.89
	0.71
	0.90
	0.95
	0.87
	0.85
	0.90
	0.75
	0.84
	0.87
	0.76
	0.86
	0.90
	0.79
	0.91
	0.95
	0.90

	Blanket bog
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(PBB)                             PA
	0.77
	0.80
	0.84
	0.51
	0.50
	0.55
	0.76
	0.81
	0.83
	0.89
	0.89
	0.94
	0.84
	0.80
	0.84
	0.78
	0.78
	0.83
	0.81
	0.82
	0.86
	0.90
	0.90
	0.94

	UA
	0.67
	0.80
	0.87
	0.49
	0.44
	0.71
	0.67
	0.81
	0.87
	0.88
	0.90
	0.94
	0.84
	0.81
	0.90
	0.70
	0.79
	0.87
	0.70
	0.80
	0.88
	0.88
	0.90
	0.94

	Woodland 
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(W)                                 PA
	1.00
	0.97
	0.99
	0.94
	0.85
	0.95
	0.99
	0.98
	0.98
	0.99
	0.98
	0.99
	0.97
	0.87
	0.99
	1.00
	0.99
	0.99
	1.00
	0.99
	1.00
	1.00
	0.99
	1.00

	UA
	1.00
	0.99
	0.98
	0.97
	0.98
	0.95
	0.99
	0.98
	0.97
	0.99
	0.99
	0.99
	1.00
	0.99
	0.97
	1.00
	0.99
	0.98
	1.00
	0.99
	0.98
	1.00
	0.99
	0.99

	Exposed Rock
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(ER)                               PA
	0.85
	0.82
	0.77
	0.84
	1.00
	0.67
	0.82
	0.84
	0.76
	0.89
	0.98
	0.81
	0.87
	1.00
	0.86
	0.82
	0.81
	0.75
	0.88
	0.83
	0.77
	0.91
	0.98
	0.83

	UA
	0.79
	0.65
	0.65
	0.10
	0.09
	0.30
	0.78
	0.65
	0.60
	0.88
	0.84
	0.79
	0.82
	0.47
	0.69
	0.82
	0.62
	0.64
	0.86
	0.73
	0.71
	0.90
	0.80
	0.80

	Disturbed ground
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(ED)                               PA
	/
	0.85
	0.55
	/
	0.64
	0.25
	/
	0.89
	0.55
	/
	0.96
	0.91
	/
	1.00
	0.87
	/
	0.93
	0.72
	/
	0.96
	0.76
	/
	0.96
	0.90

	UA
	/
	0.78
	0.97
	/
	0.13
	0.06
	/
	0.76
	0.97
	/
	0.78
	0.95
	/
	0.21
	0.86
	/
	0.76
	0.79
	/
	0.78
	0.87
	/
	0.78
	0.95

	Builtland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(B)                                  PA
	0.88
	1.00
	0.99
	0.75
	0.86
	0.85
	0.89
	1.00
	0.99
	0.97
	1.00
	0.99
	0.94
	0.95
	0.95
	0.90
	0.98
	0.99
	0.94
	1.00
	0.99
	0.99
	1.00
	1.00

	UA
	0.94
	0.98
	1.00
	0.68
	0.88
	0.91
	0.92
	0.98
	1.00
	0.99
	0.99
	1.00
	0.88
	0.93
	0.99
	0.93
	0.98
	1.00
	0.95
	0.98
	1.00
	0.99
	1.00
	1.00

	Coastland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(C)                                  PA
	0.95
	/
	/
	0.80
	/
	/
	0.95
	/
	/
	1.00
	/
	/
	0.99
	/
	/
	0.97
	/
	/
	0.99
	/
	/
	0.99
	/
	/

	UA
	0.91
	/
	/
	0.66
	/
	/
	0.91
	/
	/
	0.98
	/
	/
	0.98
	/
	/
	0.92
	/
	/
	0.97
	/
	/
	0.99
	/
	/

	Water body
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(M)                                 PA
	1.00
	0.97
	0.99
	0.94
	0.98
	0.89
	1.00
	1.00
	0.98
	1.00
	1.00
	0.99
	0.99
	1.00
	1.00
	1.00
	1.00
	0.99
	1.00
	1.00
	0.99
	1.00
	1.00
	1.00

	UA
	1.00
	0.84
	0.89
	0.95
	0.96
	0.94
	1.00
	0.89
	0.88
	1.00
	0.96
	1.00
	1.00
	1.00
	0.99
	1.00
	0.98
	0.99
	1.00
	0.98
	0.99
	1.00
	0.98
	1.00







Table S2: Level 0 classification results for the different datasets at each of the three study sites. BR – Mount Brandon, GT – Galtee Mountains, and CM – Comeragh Mountains.
	
	(i) Optical & texture
	(ii) Radar & texture
	(iii) Optical & texture & VIs
	(iv) Optical & ancillary data
	(v) Radar & ancillary data
	(vi) Optical & Radar
	(vii) Optical & Radar      (inc texture & VIs)
	(viii) Optical & Radar & ancillary data

	
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM

	Overall Accuracy (%)
	89.9
	91.4
	89.5
	67.9
	69.5
	72.5
	88.9
	91.3
	88.8
	95.1
	94.7
	94.6
	88.3
	86.3
	90.1
	90.3
	90.8
	89.9
	91.6
	92.2
	91.5
	95.5
	95.3
	95.2

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Grassland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(G)                                 PA
	0.98
	0.97
	0.93
	0.60
	0.73
	0.74
	0.97
	0.97
	0.92
	0.99
	0.98
	0.95
	0.88
	0.93
	0.92
	0.98
	0.97
	0.92
	0.97
	0.98
	0.93
	0.99
	0.98
	0.95

	  UA
	0.98
	0.96
	0.93
	0.68
	0.79
	0.74
	0.98
	0.96
	0.93
	0.99
	0.97
	0.96
	0.87
	0.87
	0.91
	0.98
	0.96
	0.93
	0.98
	0.96
	0.93
	0.99
	0.97
	0.96

	Heath
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(H)                                 PA
	0.79
	0.84
	0.80
	0.56
	0.58
	0.47
	0.78
	0.85
	0.79
	0.90
	0.90
	0.87
	0.78
	0.80
	0.76
	0.81
	0.84
	0.78
	0.82
	0.86
	0.81
	0.90
	0.91
	0.89

	UA
	0.85
	0.89
	0.71
	0.68
	0.67
	0.44
	0.83
	0.89
	0.69
	0.91
	0.94
	0.87
	0.82
	0.89
	0.74
	0.84
	0.88
	0.75
	0.87
	0.90
	0.78
	0.92
	0.95
	0.88

	Peatland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(P)                                  PA
	0.79
	0.81
	0.83
	0.54
	0.51
	0.53
	0.76
	0.80
	0.82
	0.89
	0.89
	0.94
	0.84
	0.78
	0.84
	0.77
	0.80
	0.84
	0.82
	0.82
	0.86
	0.90
	0.91
	0.94

	UA
	0.69
	0.80
	0.88
	0.45
	0.37
	0.70
	0.66
	0.83
	0.88
	0.88
	0.91
	0.95
	0.82
	0.82
	0.90
	0.72
	0.80
	0.88
	0.72
	0.82
	0.90
	0.87
	0.90
	0.95

	Woodland 
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(W)                                 PA
	0.99
	0.97
	0.99
	0.94
	0.86
	0.96
	0.99
	0.98
	0.99
	0.99
	0.99
	0.99
	0.97
	0.87
	0.99
	1.00
	0.99
	1.00
	1.00
	0.99
	1.00
	1.00
	0.99
	1.00

	UA
	0.99
	0.99
	0.97
	0.98
	0.98
	0.94
	0.99
	0.98
	0.97
	0.99
	0.99
	0.97
	1.00
	0.99
	0.97
	1.00
	0.99
	0.98
	1.00
	1.00
	0.98
	1.00
	1.00
	0.99

	Exposed Rock
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(E)                                  PA
	0.82
	0.92
	0.66
	0.89
	0.71
	0.54
	0.82
	0.87
	0.65
	0.91
	0.99
	0.99
	0.88
	0.93
	0.85
	0.81
	0.88
	0.72
	0.87
	0.90
	0.78
	0.93
	0.97
	0.87

	UA
	0.83
	0.75
	0.83
	0.10
	0.14
	0.20
	0.82
	0.74
	0.82
	0.89
	0.79
	0.97
	0.82
	0.32
	0.81
	0.83
	0.70
	0.72
	0.87
	0.76
	0.79
	0.91
	0.80
	0.88

	Builtland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(B)                                  PA
	0.90
	1.00
	0.99
	0.75
	0.87
	0.87
	0.90
	1.00
	0.99
	0.98
	1.00
	1.00
	0.95
	0.96
	0.95
	0.93
	0.98
	0.99
	0.94
	1.00
	0.99
	0.99
	1.00
	1.00

	UA
	0.93
	0.98
	1.00
	0.65
	0.86
	0.93
	0.92
	0.98
	1.00
	0.99
	0.99
	1.00
	0.86
	0.92
	0.99
	0.94
	0.97
	1.00
	0.95
	0.99
	1.00
	0.99
	1.00
	1.00

	Coastland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(C)                                  PA
	0.98
	/
	/
	0.80
	/
	/
	0.96
	/
	/
	1.00
	/
	/
	0.99
	/
	/
	0.97
	/
	/
	0.98
	/
	/
	0.99
	/
	/

	UA
	0.91
	/
	/
	0.63
	/
	/
	0.90
	/
	/
	0.98
	/
	/
	0.99
	/
	/
	0.93
	/
	/
	0.96
	/
	/
	0.99
	/
	/

	Water body
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(M)                                 PA
	1.00
	1.00
	1.00
	0.95
	0.98
	0.90
	1.00
	1.00
	0.98
	1.00
	1.00
	0.99
	1.00
	1.00
	1.00
	1.00
	1.00
	0.99
	1.00
	1.00
	0.99
	1.00
	1.00
	1.00

	UA
	1.00
	0.84
	0.89
	0.95
	0.96
	0.91
	1.00
	0.89
	0.89
	1.00
	0.93
	1.00
	1.00
	1.00
	0.98
	1.00
	0.93
	0.99
	1.00
	0.96
	0.99
	1.00
	0.98
	1.00









Table S3: Level 2 classification results (PA – producer accuracy, UA – user accuracy) for the different datasets at each of the three study sites for the independent validation. BR – Mount Brandon, GT – Galtee Mountains, and CM – Comeragh Mountains.
	
	(i) Optical & texture
	(ii) Radar & texture
	(iii) Optical & texture & VIs
	(iv) Optical & ancillary data
	(v) Radar & ancillary data
	(vi) Optical & Radar
	(vii) Optical & Radar      (inc texture & VIs)
	(viii) Optical & Radar & ancillary data

	
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM
	BR
	GT
	CM

	Overall Accuracy (%)
	81.7
	82.1
	82.8
	55.7
	56.5
	61.4
	81.1
	81.5
	81.2
	86.3
	85.7
	86.7
	75.8
	71.7
	80.3
	82.9
	81.7
	83.0
	85.1
	83.9
	85.8
	90.7
	86.1
	88.2

	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	Improved Grassland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(GA1)                         PA
	0.86
	0.87
	0.85
	0.58
	0.74
	0.80
	0.94
	0.94
	0.85
	0.89
	0.99
	0.98
	0.86
	0.86
	0.87
	0.83
	0.94
	0.87
	0.81
	0.83
	0.71
	0.88
	0.95
	0.95

	  UA
	0.94
	0.96
	0.99
	0.68
	0.75
	0.82
	0.83
	0.95
	0.97
	0.90
	0.92
	0.98
	0.87
	0.86
	0.96
	0.94
	0.95
	0.97
	0.99
	0.98
	0.99
	0.99
	0.92
	0.97

	Dry humid grassland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(GS3)                         PA
	0.78
	0.74
	0.60
	0.21
	0.05
	0.10
	0.87
	0.69
	0.60
	0.80
	0.64
	0.60
	0.66
	0.43
	0.48
	0.80
	0.69
	0.58
	0.74
	0.79
	0.60
	0.91
	0.69
	0.71

	UA
	0.87
	0.57
	0.76
	0.25
	0.09
	0.12
	0.81
	0.85
	0.74
	0.93
	0.90
	0.95
	0.72
	0.67
	0.50
	0.82
	0.83
	0.72
	0.84
	0.73
	0.51
	0.92
	0.85
	0.96

	Wet grassland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(GS4)                         PA
	0.68
	0.67
	0.67
	0.10
	0.00
	0.00
	0.58
	0.53
	0.58
	0.61
	0.80
	0.92
	0.87
	0.53
	0.58
	0.77
	0.67
	0.75
	0.73
	0.93
	0.92
	0.81
	0.47
	0.75

	UA
	0.62
	0.38
	0.25
	0.20
	0.00
	0.00
	0.68
	0.35
	0.22
	0.70
	0.57
	0.34
	0.71
	0.47
	0.19
	0.62
	0.37
	0.36
	0.76
	0.45
	0.42
	0.78
	0.33
	0.26

	Dry siliceous heath
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(HH1)                         PA
	0.59
	0.80
	0.75
	0.42
	0.25
	0.18
	0.83
	0.71
	0.75
	0.80
	0.82
	0.79
	0.48
	0.75
	0.54
	0.62
	0.80
	0.71
	0.53
	0.73
	0.77
	0.78
	0.82
	0.80

	UA
	0.80
	0.74
	0.70
	0.40
	0.15
	0.26
	0.56
	0.61
	0.70
	0.78
	0.88
	0.68
	0.63
	0.44
	0.64
	0.85
	0.61
	0.68
	0.67
	0.57
	0.88
	0.83
	0.85
	0.74

	Wet heath
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(HH3)                         PA
	0.68
	0.79
	0.52
	0.57
	0.16
	0.04
	0.59
	0.63
	0.44
	0.75
	0.80
	0.65
	0.75
	0.57
	0.56
	0.83
	0.67
	0.52
	0.76
	0.65
	0.63
	0.89
	0.76
	0.60

	UA
	0.61
	0.73
	0.71
	0.39
	0.42
	0.40
	0.72
	0.80
	0.66
	0.55
	0.70
	0.65
	0.55
	1.00
	0.74
	0.64
	0.75
	0.75
	0.74
	0.82
	0.89
	0.72
	0.72
	0.69

	Montane heath
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(HH4)                         PA
	0.71
	1.00
	0.59
	0.43
	0.00
	0.07
	0.60
	1.00
	0.59
	0.95
	0.75
	0.33
	0.43
	0.50
	0.56
	0.90
	1.00
	0.78
	0.95
	1.00
	1.00
	1.00
	0.75
	0.37

	UA
	0.68
	0.31
	0.64
	0.47
	0.00
	0.50
	0.71
	0.27
	0.70
	0.91
	0.60
	0.82
	0.60
	1.00
	0.83
	0.61
	0.50
	0.64
	0.75
	0.20
	0.90
	0.88
	1.00
	0.91

	Dense bracken
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(HD1)                         PA
	0.80
	0.75
	0.56
	0.30
	0.14
	0.06
	0.44
	0.84
	0.56
	0.90
	0.82
	0.78
	0.80
	0.43
	0.44
	0.80
	0.66
	0.56
	1.00
	0.93
	0.83
	0.80
	0.80
	0.72

	UA
	0.38
	0.85
	0.29
	0.27
	0.29
	0.04
	0.80
	0.73
	0.26
	0.69
	0.73
	0.39
	0.50
	0.49
	0.27
	0.36
	0.66
	0.37
	0.47
	0.77
	0.52
	0.80
	0.69
	0.39

	Upland blanket bog
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(PB2)                          PA
	0.73
	0.86
	0.65
	0.58
	0.61
	0.80
	0.53
	0.88
	0.65
	0.85
	0.83
	0.72
	0.67
	0.60
	0.75
	0.77
	0.84
	0.77
	0.98
	0.99
	0.98
	0.98
	0.92
	0.82

	UA
	0.51
	0.70
	0.62
	0.31
	0.40
	0.29
	0.73
	0.66
	0.59
	0.83
	0.72
	0.85
	0.57
	0.85
	0.82
	0.65
	0.72
	0.59
	0.63
	0.77
	0.63
	0.82
	0.79
	0.90

	Lowland blanket bog
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(PB3)                          PA
	0.63
	/
	/
	0.05
	/
	/
	0.71
	/
	/
	0.72
	/
	/
	0.19
	/
	/
	0.49
	/
	/
	0.77
	/
	/
	0.84
	/
	/

	UA
	0.75
	/
	/
	0.50
	/
	/
	0.63
	/
	/
	0.97
	/
	/
	0.57
	/
	/
	0.72
	/
	/
	0.87
	/
	/
	0.90
	/
	/

	Woodland 
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(W)                             PA
	1.00
	0.76
	0.98
	0.81
	0.73
	0.85
	1.00
	0.77
	0.95
	0.99
	0.81
	0.99
	0.98
	0.73
	0.95
	0.97
	0.81
	0.95
	0.98
	0.84
	0.96
	1.00
	0.83
	0.98

	UA
	0.98
	0.94
	0.95
	0.95
	0.86
	0.96
	0.98
	0.94
	0.94
	1.00
	0.95
	0.96
	0.93
	0.85
	0.93
	0.98
	0.93
	0.97
	0.99
	1.00
	1.00
	1.00
	0.94
	0.99

	Exposed Rock
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(ER1)                         PA
	0.83
	0.62
	0.78
	0.26
	0.00
	0.00
	0.75
	0.62
	0.67
	0.71
	0.85
	0.89
	0.54
	0.08
	0.56
	0.86
	0.77
	0.67
	0.98
	0.92
	1.00
	0.94
	0.92
	1.00

	UA
	0.76
	0.80
	0.47
	0.38
	0.00
	0.00
	0.69
	0.44
	0.40
	0.93
	0.79
	0.50
	0.79
	1.00
	0.45
	0.86
	0.56
	0.46
	0.89
	0.80
	0.64
	0.94
	0.92
	0.64

	Disturbed ground
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(ED1)                         PA
	/
	0.71
	0.86
	/
	0.64
	0.17
	/
	0.61
	0.86
	/
	0.68
	0.83
	/
	0.68
	0.90
	/
	0.57
	0.59
	/
	0.71
	0.90
	/
	0.75
	0.90

	UA
	/
	0.95
	0.89
	/
	0.86
	0.45
	/
	1.00
	0.89
	/
	1.00
	1.00
	/
	0.70
	1.00
	/
	0.89
	0.85
	/
	0.95
	1.00
	/
	0.95
	0.96

	Builtland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(B)                              PA
	0.97
	0.93
	0.99
	0.81
	0.93
	0.86
	0.69
	0.92
	0.98
	0.97
	0.95
	0.96
	0.95
	0.98
	0.95
	0.92
	0.90
	0.96
	0.98
	0.93
	0.97
	0.95
	0.96
	0.99

	UA
	0.77
	0.98
	0.98
	0.39
	0.57
	0.69
	1.00
	0.98
	0.99
	0.73
	0.96
	0.98
	0.56
	0.63
	0.82
	0.81
	0.97
	0.98
	0.91
	0.98
	1.00
	0.92
	0.98
	0.98

	Coastland
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(C)                              PA
	0.88
	/
	/
	0.79
	/
	/
	1.00
	/
	/
	0.90
	/
	/
	0.85
	/
	/
	0.90
	/
	/
	0.85
	/
	/
	0.85
	/
	/

	UA
	1.00
	/
	/
	0.86
	/
	/
	0.98
	/
	/
	0.96
	/
	/
	0.93
	/
	/
	0.98
	/
	/
	0.95
	/
	/
	0.91
	/
	/

	Water body
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	(M)                             PA
	0.98
	0.91
	0.91
	0.98
	0.82
	0.85
	1.00
	1.00
	0.88
	0.99
	0.73
	0.94
	0.98
	0.91
	0.94
	0.98
	0.82
	0.99
	0.99
	0.91
	1.00
	0.98
	0.91
	1.00

	UA
	1.00
	0.77
	0.97
	0.97
	1.00
	0.94
	1.98
	0.85
	0.95
	1.00
	1.00
	0.98
	0.96
	1.00
	1.00
	1.00
	0.75
	0.92
	1.00
	1.00
	1.93
	1.00
	1.00
	0.96
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